**ATTENTION**

**SAFE USE OF THE LOCAL EXHAUST VENTILATION SYSTEM**

10% OF THE DUCTS **MUST BE CLOSED** TO ENSURE ADEQUATE EXTRACTION